**Move operations of the railroad tracks**

| **Activity** | **Hazard** | **Consequences** | **Risk Rating** | | | **Existing controls** | **Risk Rating with control** | | | **Result** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **L** | **S** | **R** | **L** | **S** | **R** |
| - Rig Move Operations (Trucks passing through Railroad tracks). | - Dropped load.  - Damage to equipment.  - Personnel injury-Death.  - Break down for trucks on the railroad | - Dropped load  - Electrical Short  - Train and trucks crash. | 4 | 5 | 20 | * Pre-Job safety meeting to be held with ECDC Crews. * Pre-Job safety meeting with the drivers to ensure that the all the loads are secured well. * Work group supervisor. * Moving the trucks in a convey. * Good communication between HSE ECDC and HSE KEE during the moving all loads. * Competent Trucks Drivers. | 2 | 2 | 4 | L |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |